**MM-EC1500RT2U** ENCOMPASS UPS 1500 VA 1350 W

* 1500VA/1350W 120 VAC true on-line, double-conversion, extended runtime rack/tower UPS designed for critical, power-sensitive electronic environments
* True online, double-conversion technology
* Compact case design, (only 2U for all models), for high density rack installations
* Flexible installation format: Rack/Tower
* Rackmount ears come attached to UPS
* Easy-to-read LCD display
* 0.9 output power factor
* Highly-efficient, Economy Mode option
* Output receptacle control with 2 banks
* Independent Battery Bypass – allows the UPS to provide voltage regulation and spike/surge protection either with dead batteries or without batteries
* Hot-swappable battery replacement
* Cold Start capable
* Automatic internal bypass
* Simultaneous USB and RS232 communications
* Compatible with Minuteman’s SentryHD software
* SNMP compatible (with optional card)
* Dedicated EPO port
* Tool-less battery replacement design
* 1Gbit RJ45 network protection
* Full three-year warranty (including batteries)
* Green UPS design (RoHS and Energy Star compliant)