**MM-ETR1000LCD** Entrust LCD Series UPS 1000VA/600W

* 1000VA Line Interactive AVR Compact Tower UPS
* Tool-less battery panel allows for easy-access setup and maintenance
* Monitor and manage via USB and SentryHD Software
* LCD control panel displays: unit status, load and battery meters, numeric display, scroll button, alarm silence button, on/off/test button
* Regulates output voltage for protection against spikes, surges, brownouts, and blackouts
* Compact form factor ideal for tight installs
* Apparent Output Power: 1000VA
* Active Output Power: 600W
* Equipment Protection Policy: Up to $75,000 insured by Minuteman
* Voltage Range: 90VAC-140VAC
* Frequency Range: 60Hz ±6Hz
* Efficiency: >96% (full load)
* Voltage: 120VAC
* Full Load Runtime (non-linear): 3 minutes
* Half Load Runtime (non-linear): 12 minutes
* Hot Swappable Batteries
* Typical Recharge Time: 8 hours to 90% from full load discharge
* Battery Type: sealed, non-spillable, maintenance-free, value-regulated lead-acid