**MM-PRO1500RT2U** LINE INTERACTIVE 1500VA 1050 WATTS UPS

* 1500VA/1050W 120 VAC line-interactive UPS with 8 battery backup/surge outlets, USB communication port, SentryHD power management software and diagnostic software, and fax/modem/network line surge protection
* Protection from Spikes, Surges, Brownouts, and Blackouts
* Buck and boost Automatic Voltage Regulation (AVR) function
* All outlets are battery and surge-protected
* RJ11 / RJ45 spike/surge protection for phone/fax/ modem/network connections (1Gb)
* Coax protection for satellite/cable
* Rack/tower Installation
* 2U rack height or wall mounting with optional kit
* Minuteman SentryHD Software
* Automatically saves and shuts down unfinished or open applications programs
* Powers down your devices during blackouts
* Provides comprehensive power monitoring
* USB Communications
* No special USB drivers are required. The USB is automatically recognized by Microsoft® Windows® as HID-compliant devices – similar to a mouse or a keyboard.
* SNMP Compatible
* Each PRO-RT unit can be managed on a network with the addition of an optional SNMP management card. (NC models includes a pre-installed network card)
* Fax/Modem/Network/Coax Line Protection
* The PRO-RT UPS provides a low cost means of protecting fax/modem/network lines.
* Independent Battery Bypass
* Provides voltage regulation with surge and spike protection even when batteries are weak or dead.
* Auto-restart
* When power returns after an extended outage and the batteries have been fully drained, the UPS automatically restarts and provides power to attached devices if acceptable AC is present.