**MM-MMS660S** 6 Outlet Wall Tap Surge Suppressor, 540J

* Slimline Series 6 Outlet Wall Tap Surge Suppressor
* Six grounded outlets
* Wall-tap anchors to outlet using included screw
* High visibility green LED protection indicator
* Attractive and functional low-profile design
* UL 1449, 1363 certified
* $50,000 connected equipment protection from Minuteman
* Electrical Rating: 15A, 120V, 1800 Watts
* Joule Rating: 540
* UL Clamping Voltage: 500V
* Maximum Peak Current: 36,000A